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1. Immediately notify an electrician when a dangerous electrical condition is identified.
2. Do not permit the use of electrical installations that do not comply with technical requirements.
3. Only electricians shall perform maintenance and repair on electrical equipment and circuits.
4. Repairs shall not be performed on equipment or systems that have not been de-energized.
5. A warning sign shall be placed on the panel or switch from which the power has been disconnected.
6. Inspect the electrical tool and its cable before use.
7. Never pull on the cable to disconnect the plug from the socket.
8. Do not route cables over hot surfaces or sharp edges.
9. Do not use defective plugs or sockets.
10. When defective equipment is identified, immediately remove it from service.
11. Appropriate warning signs shall be posted on all electrical panels and power sources.
12. Only authorized personnel shall enter areas containing the main electrical installation.
13. Except during repair, electrical panel covers shall be kept closed.
14. Chemicals, flammable, and combustible materials shall not be stored near electrical panels.
15. Materials shall not be stored in a way that blocks access to electrical panels, control boxes, or emergency switches.
16. All panels shall be grounded, and hand tools without proper grounding shall not be used.
17. Hand tools shall not be placed where they may fall.
18. Measures shall be taken to prevent electrical cables from causing trips and consequent falls.
19. Protective equipment shall be used when working with hand tools.
20. Do not reach excessively while working with hand tools. Keep your feet firmly and securely positioned.
21. When not in use, first switch off electric hand tools using the on/off switch and then unplug them.
22. After completing work, do not keep your finger on the hand tool trigger.
23. Replace defective or unsafe tools with new ones.
24. When working at height, secure hand tools against falling. Do not leave hand tools randomly in passageways or walkways where personnel may trip over them.
25. Do not throw tools from one place to another.
26. Keep tools clean to prevent slipping from the hand; do not allow grease or oil to contaminate them.
27. Do not use the cable of electric hand tools to suspend or pull the tool.
28. [bookmark: _GoBack]Do not stand on wet or damp floors when using electrical tools.
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