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1. Ensure that all windows, exterior mirrors, and exterior light lenses are clean.
2. Walk around the vehicle and visually inspect it for any leaks.
3. Check the operation of the brakes and steering.
4. Check the gauges.
5. Check tire pressure and condition.
6. Use the personal protective equipment provided to you.
7. Immediately report any defect to your responsible supervisor and ensure that all necessary repairs and inspections have been completed.
8. Ensure that all steps are free of grease, oil, snow, and ice.
9. Fasten the safety belt.
10. Even for short periods, ensure adequate ventilation when operating the vehicle indoors. Do not allow exhaust gases to cause poisoning.
11. Do not engage in other activities while working.
12. Do not smoke during work.
13. Thoroughly inspect the work area before starting work. Do not begin until other employees in the area have left the work area.
14. In areas where visibility is inadequate or outside the field of vision, request a signaler. The signaler shall stand where the operator can easily see them and direct the work using predetermined signals.
15. Obey every stop signal given during work, regardless of who gives it.
16. Pay attention to power transmission lines within the work area. Keep the distance between the vehicle and power lines greater than the required clearance distance.
17. Keep vehicle accessories and auxiliary equipment (tow rope, reflector, first-aid kit, fire extinguisher, etc.) securely stored, sound, clean, maintained, and ready for use at all times.
18. Do not leave for a task without completing the 'VEHICLE TASK FORM'.
19. Before starting any repair on pressurized hydraulic lines (hoses/pipes), ensure that pressure has been released from the hydraulic hoses.
20. Never remove or install hydraulic lines (hoses/pipes) while the machine is running.
21. Check whether the control levers and pedals perform their functions.
22. Start maintenance, repair, or cleaning only after stopping the machine.
23. Ensure that the reverse alarm is always operational.
24. Even during short stops, the operator must ensure that no person is under or around the vehicle.
25. Before using the machine, read and understand the operation and maintenance manual and keep it readily available.
26. Keep maintenance and inspection records regularly and keep the maintenance card in the vehicle at all times. Read the maintenance and repair booklet and ensure periodic maintenance is performed according to the vehicle's specified operating hours by following maintenance and inspection records.
27. Report defects and deficiencies observed on the vehicle to the authorized persons.
28. When stopping the engine, always apply the parking brake.
29. After maintenance is completed, perform a final external inspection of the vehicle (oil or water leaks, flat or deflated tires, hoses).
30. Do not rest or sleep under, beside, or at the step and slope edges of the vehicle.
31. Do not wear wide or loose clothing or trousers during maintenance. Check the vehicle's antifreeze before winter.
32. Leave the operator cabin only when the engine is stopped and while facing the cabin with three-point contact.
33. Check that the lights, beacon, brake lights, and turn signals are operational.
34. Before starting work, ensure that unauthorized persons are not present in the work area.
35. Check the blade bolts and blade joint connection bolts.
36. Inspect the grader's running gear and tighten any loose bolts.
37. Replace the grader blade safety pin only when the engine is stopped.
38. Engage and disengage the differential lock on vehicles equipped with one only when the steering is straight and the vehicle is stationary.
39. Personnel assigned as operators and entrusted with a vehicle shall keep the vehicle maintained, clean, fueled, and ready for duty at all times.
40. Do not allow unauthorized persons to ride in the vehicle during travel.
41. During travel with graders, no one other than assigned personnel may be present.
42. Graders shall be operated only by persons with the appropriate driving license. Operators are responsible for operating the grader safely under all weather conditions.
43. Maintain a safe distance from the articulated joint area while the vehicle is operating to prevent crushing.
44. In winter, fit tire chains to prevent wheel spin.
45. Keep a dry chemical powder or foam fire extinguisher available for fire protection.
46. Remember that compliance with Occupational Health and Safety rules is mandatory during all operations.
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