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The forklift shall be operated only by authorized personnel who have received forklift operator training.
Immediately report visible defects or required repairs to the unit supervisor.
Always follow forklift operating rules and safety precautions and heed all warnings.
Do not operate the forklift before sitting in the operator's seat. Do not extend your arms, legs, or head outside the operator compartment. Keep hands and feet away from the forklift mast.
Avoid sudden maneuvers at high speed with the forklift; do not make sudden stops or starts.
Use the horn to warn others and reduce speed when turning, entering or leaving buildings, and when near people.
Never operate the forklift with wet hands or footwear. Do not operate the levers with wet hands.
Do not carry or lift anyone on the forklift forks.
Do not allow other people to ride on the sides of the forklift.
Never operate the forklift without the operator guard and load backrest.
Carry the load with the mast tilted backward.
Do not lift or carry unsafe or unstable loads.
Load the material so that its center of gravity is balanced. Unbalanced loads increase the risk of overturning.
Adjust the fork spacing according to the load's center of gravity and always carry the load properly stacked.
Always use a pallet of suitable size.
Keep the forks as widely spaced as possible under the load.
Distribute the load equally over both forks and never carry a load using only one fork.
Never overload. Always load within the tonnage recommended for the forklift.
Never add a counterweight to the forklift. Heavy loading may cause the forklift to overturn.
Do not operate the forklift on loose ground. In particular, do not exceed limits such as the maximum permitted load for the ground conditions, lifting capacity, or ceiling height.
Do not operate the forklift on slippery surfaces. Accidents may occur on sand, gravel, ice, or muddy ground and may result in overturning. If operation is unavoidable, proceed slowly.
Do not allow anyone to pass or stand under the forklift load or lifting mechanism. The load may fall and cause injury or death.
Excessive stacking or raising the load will obstruct visibility. Do not operate the forklift with the load raised or the mast elevated. The forklift may overturn and cause damage, injury, or death.
Do not move the forklift if the load is higher than the load backrest.
Take care to prevent the load from falling during loading.
Carry the load with the forks as low as possible and the mast tilted backward. This improves forklift stability and provides better visibility.
Never raise a loaded forklift with the mast tilted forward, and do not tilt the mast forward while the load is raised. This can cause the forklift to tip forward.
When the forklift begins to overturn, do not attempt to jump out. Sit in the seat and hold on firmly to survive.
When ascending ramps, always travel forward; when descending, travel backward.
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