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1. The area in front of the fire hose cabinet shall always be kept clear. Panels, cabinets or other objects shall not be placed in front of it.
2. One end of the hose inside the fire hose cabinet shall be connected to the valve and the other end to the nozzle. Hoses shall always be kept ready for use.
3. The inside of the fire hose cabinet shall always be kept clean. Paper, cleaning cloths or other materials shall not be stored inside.
4. Fire hose cabinets shall not be used for purposes other than firefighting.
5. The responsible personnel shall know the location of the building’s main water valve.
6. When the valve is opened, the responsible personnel shall check monthly whether sufficient water pressure reaches the hoses and record the results regularly on the inspection form.
7. Used textile-type hoses shall be dried, folded in half lengthwise and wound onto the reel in such a way that they can be easily unwound without catching or becoming tangled.
8. There shall be no water leakage inside the cabinet when the valves are opened. If defective hoses, clamps or gaskets are identified, they shall be reported immediately to the school administration for replacement.
9. The school administration is responsible for the proper use and periodic maintenance of the fire hose cabinets.
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