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1. The saw shall be inspected before starting work.
2. Defective or cracked saw blades shall not be used.
3. The saw blade shall always be kept properly tensioned and adjusted using the tensioning mechanism.
4. The saw shall be used only for its intended purpose.
5. The appropriate saw blade shall be installed for the cutting operation. Fine-toothed blades shall be used for cutting hard and dry wood, while coarse-toothed blades shall be used for cutting soft and damp wood.
6. After starting the machine, cutting shall not begin until the machine has reached its normal operating speed.
7. Check that there are no nails, stones or other hard objects in the material to be cut.
8. During cutting operations, hands shall be kept at a safe distance from the saw blade.
9. The saw shall not be used if the ON/OFF switch is not functioning properly.
10. Wear close-fitting clothing and fold sleeves inward.
11. Appropriate safety goggles, a face shield and a dust mask shall be worn during work.
12. In the event of any jamming, the saw blade shall not be touched until the motor has been stopped, even if the band saw itself has stopped.
13. The motor shall be switched off before replacing the saw blade.
14. In the event of a malfunction, stop the saw motor immediately and notify the relevant personnel.
15. Band saw blade connections and related components shall be inspected and checked at least once a month.
16. Saw guards shall not be removed except for maintenance and repair purposes.
17. Guards removed during maintenance or repair shall be reinstalled before work is resumed.
18. The safety of people in the surrounding area shall be given as much importance as your own safety.
19. Machines with defective switches shall not be operated.
20. Wear a work apron, and fold the apron sleeves inward.
21. Any situation that is contrary to occupational health and safety requirements shall be immediately reported to the relevant personnel.
22. The machine shall be cleaned after completing work.
23. Chips and dust on the machine shall be cleaned using a brush or compressed air.
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