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Full compliance with the requirements specified in the project and specifications is essential in all applications.

Brick and Blockwork

1. Ensure that the mortar thickness is neither less nor greater than required.
1. Horizontal and vertical joints shall be of the same thickness, and vertical joints shall be staggered.
1. Bricks and blocks shall have a low water absorption rate.
1. If the wall surface will be plastered, the joints shall be flush with the surface; if it will not be plastered, they may be recessed or protruding.
1. In hot weather, the wall surfaces shall be wetted periodically after completion to prevent mortar cracking and cracks caused by water loss.
1. The wall surface shall be kept level and plumb to reduce plaster waste.

Plastering Works

1. Plaster shall be prepared from a mixture of water, cement, plaster sand, and lime. The lime shall be fully slaked, and the sand shall be neither too fine nor too coarse (of the required grading).
1. Before plastering begins, the wall shall be divided into screed sections. The sections shall be marked with manually applied vertical strips of plaster 20–25 cm wide.
1. Plaster thickness shall be checked frequently.

Painting Works

1. The paints specified in the project/specifications shall be used, and trial applications in alternative colours shall be made and submitted to the supervising engineer for approval.
1. Spray painting on exterior surfaces shall be avoided in windy weather.


Cladding Works

1. Cladding works include covering elements such as walls, roofs, and floors with prefabricated building components.
1. Application/detail drawings shall be prepared to ensure high-quality cladding and minimize waste.
1. Attention shall be paid to joint details to ensure visual integrity.
1. Detailed drawings shall be prepared for sections where different claddings meet, and potential problems likely to arise during application shall be resolved at this stage.

Waterproofing and Insulation Works

1. The project details shall be compared with the supplier’s details; any differences shall be identified and resolved before the application stage.
1. Application details and specifications shall be followed strictly. Deficiencies or defective workmanship in insulation works are very costly and generally impossible to rectify.

Joinery Works

1. Detail drawings shall be prepared and any problems that may arise during application shall be resolved at this stage.
1. A sample section shall be prepared before application and approved by the supervising engineer.
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