


	[image: ]
	YOZGAT BOZOK UNIVERSITY 
WELDING MACHINE OPERATING INSTRUCTIONS
	
[bookmark: _GoBack]Documan Number: KYT-TLM-032
Publication Date: 20.08.2024
Revision Date:: 
Page No: Page 1 / 1




1. Do not operate the welding machine by installing it next to, near, or on top of flammable or combustible materials.
2. Do not block the machine's air intake openings.
3. Prolonged operation may cause the machine to overheat and subsequently malfunction. Therefore, allow the machine to cool at appropriate intervals.
4. Do not touch the moving parts of the machine.
5. Do not remove the cover, panels or guards under any circumstances.
6. If the machine malfunctions in any way, notify the mechanical maintenance department.
7. During work, you shall wear a welding helmet, gloves, flame-resistant safety clothing and the personal protective equipment provided to you according to the nature of the work.
8. Check the electrical connection before starting work. If there are worn or damaged cables, notify the electrical team.
9. During welding, never wear a necktie or loose clothing and do not wear jewelry such as a wristwatch, chain or ring.
10. Never inhale the gases released during welding.
11. Leave electrical work to authorized personnel.
12. Make sure that the chassis cables are not bare or stripped.
13. Start work only after ensuring that the machines are properly grounded.
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