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1. The cutting drill bit shall be selected according to the type and thickness of the material to be drilled.
2. Always take precautions to ensure that your fingers and hands do not remain in front of the drill; work carefully.
3. Ensure that the drill bit is properly seated, centered, securely fixed, and not loose. Do not start work without checking the condition of the drill bit.
4. To protect your body and/or hands, hold the hand drill correctly and use its designated handles (to prevent slipping); do not work with the drill too close to your body.
5. Do not start work without suitable positioning when there is no adequate support, when you cannot work in a stable and safe manner, or when working on poor surfaces.
6. For bench work, secure the hand drill to prevent rotation, slipping, movement of the workpiece, etc.
7. Always switch off the hand drill and unplug it when you have finished using it, when changing the drill bit, or when checking any other part.
8. When drilling small parts, use a vise; if this is not possible, use a suitable fixing device. The workpiece shall be securely fixed.
9. Check that the workpiece fixture and vise are securely fastened to the drill press table.
10. Wear safety goggles and a face shield, taking into account that chips may be ejected while drilling.
11. Gloves, necklaces, bracelets, rings, or ID tags shall not be worn when working with rotating machinery.
12. The sleeves and cuffs of work clothing shall be elasticated; personnel operating a drill shall not wear loose or dangling clothing.
13. Ensure that the hand pressing the material against the rotating drill and the other supporting hand remain firm and stable.
14. When working on drill presses, wear steel-toe safety footwear to protect against falling parts.
15. If excessive heat is generated during drilling, use coolant or oil.
16. The machine shall be properly grounded.
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