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1. All belts, pulleys, and shafts shall be properly guarded.
2. Check that the shaft adjustment mechanisms are functioning properly.
3. The machine must be properly grounded.
4. The cutter or cutters shall be covered with a fixed guard to prevent flying parts and chips.
5. Check and clean the guards and clamping devices.
6. The coolant shall be directed toward the side away from the workpiece.
7. The workpiece to be machined must be securely fixed to the machine.
8. Ensure that the cutter and spindle are securely fastened.
9. Check the sharpness of the cutters.
10. When the machine is stopped, chips must be removed using a brush.
11. Never use the tool with a damaged power cord.
12. Do not use the tool in the rain or in wet areas.
13. Always keep the cable behind the tool.
14. Hold the tool only by its insulated handle.
15. Always hold the tool firmly with both hands while working and ensure that your working position is safe.
16. Before starting to use the tool, check that the milling cutter is securely seated in its proper position.
17. Never perform milling operations on metal parts or objects containing nails or screws.
18. Keep your hands away from the rotating milling cutter (milling bit or milling cutter).
19. Wear protective gloves when installing or changing milling cutters.
20. Adjust the milling depth only when the tool is switched off.
21. Personnel working on this machine must not wear loose or dangling clothing, ties, long-sleeved garments, or similar items during operation.
22. Personnel working on milling machines shall pay maximum attention to general hygiene rules to protect themselves against skin diseases and inflammations caused by machine oils.
23. Operators must use appropriate Personal Protective Equipment (PPE), such as safety goggles, face shields, gloves, masks, steel-toe safety footwear, coveralls, etc.
24. Do not attempt to calibrate or measure workpieces while the machine is in motion.
25. Do not leave hand tools on the machine table.
26. Machine guards and protective equipment must never be removed.
27. Clean the machine of chips and dust at the end of each working day.
28. In the event of a machine malfunction, the employee must not attempt to intervene.
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