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1. If the load obstructs your view, ask a spotter to guide you.

2. When transporting loose loads, use a pallet.

3. Do not transport loads on slopes exceeding 1%.

4. Use the pallet truck only on flat and firm surfaces.

5. When transporting a load, stand on the handle side of the pallet truck.

6. Do not transport people using the pallet truck.

7. When leaving the pallet truck unattended, lower the forks to their lowest position.

8. Place the load evenly and securely on the forks.

9. Never lift a load using only one fork or the tip of a fork.

10. Do not load the pallet truck while the forks are in the raised position.

[bookmark: _GoBack]11. Never stand underneath a raised load or within the hazardous area around a raised load (600 mm).
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