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1. The salt spreader vehicle shall only be operated by authorized personnel. Unauthorized use is strictly prohibited.

2. Do not climb onto the salt spreader while the vehicle is moving.

3. If it is necessary to climb onto the salt spreader, take all necessary safety precautions before doing so.

4. Comply with all traffic rules. Do not exceed the specified speed limits.

5. Use the required personal protective equipment (PPE).

6. Exercise caution around pressurized hoses.

7. Ensure that the warning beacon is functioning properly.

8. Lubricate the points specified in the maintenance manual at regular intervals.

9. Check bolt connections regularly. Tighten any loose bolts.

10. To prevent accidents, carry out maintenance and repair of the salt spreading equipment only when the vehicle engine is switched off and the hydraulic system is deactivated.

11. At the end of each winter season, inspect all areas where corrosion may have occurred.

12. Take the necessary safety precautions around the salt spreader to prevent possible accidents.

13. Check hydraulic hoses, pipes and valve blocks for oil leaks.

14. Clean the salt spreader at regular intervals.

15. Never disconnect or remove fittings, hydraulic pumps, motors, valves or cylinders while the system is under pressure.

16. Switch off the hydraulic power unit and stop the engine before carrying out maintenance or repair work.

17. In the event of any malfunction, immediately notify the authorized personnel and ensure that all necessary repairs and inspections have been fully completed.

18. Read the Material Safety Data Sheets (MSDS) for all chemicals you use or store, and learn about their hazards and the safety precautions to be taken.

19. Keep the Material Safety Data Sheets readily accessible.

20. Do not engage in any other activity while working. Smoking, eating or drinking during work is prohibited.

21. Obey every stop signal, regardless of who gives it.

22. Check that the control levers and pedals are functioning properly.

23. Even during short stops, the operator shall ensure that no person is underneath or around the vehicle. The vehicle shall not be moved without first checking the surroundings. Use a spotter when necessary.

24. Keep maintenance and inspection records regularly and keep the maintenance card in the vehicle at all times.

25. Before reversing, ensure that the maneuvering area is clear and safe.
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