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1. Check that there are no nails, stones, or other foreign objects on the workpiece. If necessary, remove them using a wire brush.
2. Check the location and proper operation of the emergency stop buttons.
3. Ensure that the machine is properly grounded.
4. Ensure that guards are installed on moving parts such as belts, pulleys, and gearboxes.
5. Remove any tools, equipment, materials, or other items that are not required from the machine, work area, and floor to prevent tripping and falling.
6. Do not operate the machine if its electrical cables are unsuitable, stripped, or damaged.
7. Do not wear loose or hanging work clothes. Do not wear gloves or neckties while working. Do not wear wristwatches, chains, rings, or other accessories.
8. **NEVER** operate the machine with blunt or damaged blades.
9. Do not start working until the machine has reached its normal operating speed.
10. When pushing the workpiece, do not pass your hands over the blades.
11. Stand firmly on the left side of the machine while working.
12. Check regularly that all adjustment and clamping mechanisms are secure, particularly the blade fastening bolts.
13. Do not set the cutting depth to more than **2 mm on wide surfaces and 5 mm on narrow surfaces**.
14. Wait until the machine has come to a complete stop before cleaning away shavings.
15. During operation, be careful to prevent the workpiece or shavings ejected from the workpiece from striking you.
16. Do not attempt to remove shavings with your hands.
17. When necessary, carefully use a shaving hook.
18. If shavings interfere with your work, switch off the machine before cleaning and removing them from the workpiece. Use an air gun to remove small shavings from the machine table.
19. Adjust the fence so that it forms a right angle with the table.
20. **The protective equipment/guards of the machines must never be removed.**
21. In the event of a machine malfunction, the operator must not attempt to intervene. Report the malfunction to the authorized personnel.
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