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1. The machine must not be operated or used without the supervision of the responsible personnel. 
2. Before starting and while operating the machine, the operator must ensure that they are at a safe distance from other people and objects. 
3. Maximum attention must be paid during operation to prevent hand or foot injuries. 
4. Since the exhaust gases emitted by the machine are toxic, it must not be operated in areas without adequate ventilation. 
5. Do not refuel while the engine is running. Keep away from open flames. 
6. Do not operate the machine without wearing the required occupational health and safety equipment. 
7. Remove stones, wires, pieces of glass, bushes, and metal objects from the work area. 
8. Do not operate the machine if the safety devices are not in good working condition (Stop/Engine Safety Lever). 
9. If the machine strikes an object during operation, stop the machine and check for damage. 
10. Do not operate the machine if the ground is wet. 
11. Do not operate the machine if the tiller blades are not sharp. 
12. Do not operate the machine if the Stop/Engine Safety Lever is not functioning. 
13. If you lose your balance while operating the machine, release the Stop Lever and allow the machine to stop. 
14. Operate the machine in daylight and in adequately illuminated areas. 
15. Never leave the machine unattended while it is running. 
16. Do not operate the machine on excessively steep or sloping terrain that is unsuitable for the machine. 
17. Do not overfill the fuel tank to avoid the risk of fire.
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