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1. Personnel working with an angle grinder shall not wear loose or hanging clothing, ties, long-sleeved garments or similar clothing during work. Tight-fitting clothing shall be worn, and sleeves shall be folded inward only. Work shall not be carried out while wearing clothing with loose sleeves or loose pockets.

2. If the workpiece becomes detached or is thrown from its fixed position, do not attempt to catch it by hand; stop the machine immediately.

3. Check the condition of the angle grinder’s cable and plug.

4. Ensure that the grinding wheel is properly mounted and tightened with the appropriate wrench, that the wheel is dry and free from cracks, and that the wheel guard is properly installed.

5. Protruding parts of workpieces mounted on rotating tables shall be adequately enclosed with suitable guards.

6. While the workpiece is being processed, chips located at the cutting tool edge shall not be removed by hand. Guards or shields shall be provided to prevent coolant from splashing.

7. All portable or stationary grinding and cutting machines shall be equipped with suitable grinding wheel and cutting disc guards.

8. The machine shall under no circumstances be operated while maintenance or repair work is being carried out.

9. An angle grinder produces sparks. If flammable or combustible materials are present in the work area, they shall be removed and the necessary safety precautions shall be taken.

10. Necessary precautions shall be taken to prevent sparks and flying particles generated during work from reaching nearby workers or combustible materials.

11. Chips shall not be swept up by hand; suitable brushes shall be used for this purpose.

[bookmark: _GoBack]12. The angle grinder guard must always be installed. Working without the guard and without safety goggles shall be prevented.

13. Check that the angle grinder’s ON/OFF switch is in good working condition. The grinder shall start when the button is pressed with a finger and stop when the finger is released.

14. Use properly grounded electrical equipment.

15. Grinding wheels and cutting discs are used with angle grinders. Pay attention to the type of wheel being used and do not use it for an unsuitable operation. Grinding wheels shall be used for grinding, and cutting discs shall be used for cutting.

16. After completing the work, unplug the angle grinder from the electrical outlet.

17. After completing the work, do not leave the angle grinder on the floor; place it in its designated storage location.

18. The permissible rotational speed is indicated on grinding wheels. The rotational speed of the angle grinder shall be lower than the maximum permissible speed of the wheel.

19. When working with a cutting disc, the disc shall be perpendicular to the material being cut and shall not be tilted during cutting.

20. Do not apply excessive pressure to the material with the disc in an attempt to increase cutting performance.

21. Do not place the angle grinder on the floor until the wheel has come to a complete stop.

22. The angle grinder shall only be operated by the person authorized and responsible for its use.

23. When taking a break from work or when changing the wheel, unplug the angle grinder from the electrical outlet.

24. Do not perform sharpening or grinding by laying the angle grinder on the floor. The workpiece to be ground shall always be securely fixed.

25. Do not operate the angle grinder with wet or oily hands or gloves.

26. When working with an angle grinder, safety footwear with protective toe caps, a face shield/safety goggles, assembly or welding gloves, and hearing protection shall be worn.

27. The angle grinder shall be operated below elbow level. It shall not be operated above head level.

28. Do not leave the tightening wrench or any other tools on the angle grinder.
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