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1. 1. Gloves shall not be used when carrying out repair, maintenance, or servicing of machines and machine tools with rotating parts.
2. 2. During maintenance and repair, a 'CAUTION – MAINTENANCE IN PROGRESS' sign shall be placed on the start/operation button and at the electrical switch or plug supplying power to the equipment.
3. 3. Maintenance or repair shall not be performed on a running machine.
4. 4. Before starting maintenance, stop the machine and disconnect the electricity.
5. 5. Obtain assistance from the electrical team for work involving the machine's electrical components.
6. 6. If there is a workshop designated for maintenance, move the vehicle or machine there; otherwise, move it to a quiet area with low work activity.
7. 7. If chemicals are used during maintenance, act in accordance with the MSDS and receive training concerning the chemical.
8. 8. If a pressurized cylinder is used during the work, secure the cylinders and keep them away from heat. Use the required personal protective equipment (gloves, goggles, mask, boots, safety footwear, hearing protection, apron, etc.) throughout maintenance and repair.
9. 9. Hand tools used shall be sound and safe; defective or damaged tools shall not be used.
10. 10. At the end of the work, check and confirm that damaged or removed systems, cables, and other components have been correctly reinstalled.
11. 11. Inform the operator of any changes made to the machine, machine tool, or system during maintenance and repair.
12. 12. Record important findings identified during maintenance and take them into account during subsequent inspections.
13. 13. Maintenance and repair work shall be performed by competent persons.
14. 14. Reinstall all guards removed during the work when the work is completed.
15. 15. Pressure vessels and boilers shall not be repaired under pressure. Disconnect tanks, boilers, or reservoirs to be repaired from other tanks and reservoirs.
16. 16. Containers holding flammable or explosive substances shall be cleaned before maintenance or repair.
17. 17. For maintenance and repair work at height, a platform or scaffold shall be installed, and a safety harness and hard hat shall be used.
18. 18. The insulation of portable cables used shall be intact.
19. 19. Portable electrical equipment shall be 24 volts.
20. 20. Before repairing moving parts such as belts, pulleys, gears, couplings, and fans, stop the machine and disconnect the electricity.
21. [bookmark: _GoBack]21. Remove flammable and explosive materials from the surrounding area before starting maintenance work.
22. 22. The work area shall be adequately illuminated.
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