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1. A hard hat shall be worn without exception wherever head protection is required.
2. All hard hats shall always be inspected for breaks, cracks, wear, electrical hazards, or contact with chemicals.
3. There shall be at least 32 mm of clearance between the top of the hard hat and the head.
4. During use or storage, hard hats shall be protected in accordance with their characteristics.
5. Hard hats shall be made of materials that are not adversely affected by acids, chemicals, or paint.
6. Hard hats shall be washed in 60°C hot water with a mild detergent and rinsed with hot water.
7. Hard hats used by personnel performing electrical work shall have no holes or metal parts and shall not be manufactured or purchased with water-retaining channels or similar features on the outer surface.
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