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1. Materials weighing more than 25 kg shall not be carried by one person alone on the construction site. Work gloves shall be worn while carrying loads, and the load shall be checked for nails, sharp points, and sharp edges.

2. Pay attention to the ground while carrying loads. Do not carry loads in a way that obstructs your field of vision. When necessary, seek assistance from a guide.

3. Long materials shall be carried horizontally and at an appropriate height. Pay attention to nearby power lines and electrical panels.

4. Before starting work, drivers and operators shall inspect their vehicles. They shall not operate a vehicle if it has any defects or unsafe conditions. Before entering a vehicle, they shall check that there is no one underneath it.

5. No machine or vehicle shall be operated by an unauthorized person without the required driving/operator license, and no one shall be pressured to do so.

6. Operators and drivers are responsible for the periodic maintenance and inspections of their machines and vehicles and shall report any issues to the authorized persons in a timely manner. Vehicles that have not undergone the required technical inspection/periodic inspection shall not be used.

7. During operation, no person other than the operator shall be allowed on the machines. In particular, passengers shall never be carried on the fenders or outside the cab of tractors or similar vehicles.

8. All machinery, vehicles, and transport vehicles shall comply with the 20 km/h speed limit within the construction site.

9. Warning systems such as lights, turn signals, horns, and reverse alarms shall be kept in working condition.

10. Parking outside designated parking areas and bringing private vehicles into the construction site are prohibited.

11. A signaler shall always be present during reversing maneuvers, and operators shall maintain visual contact with their signalers.

12. Loads exceeding the maximum load capacity shall not be transported. Ensure that loads do not extend beyond the vehicle during transportation.

13. Transporting people with any load-carrying vehicles or construction machinery, both within and outside the construction site, is strictly prohibited.

14. Vehicles and machinery shall not be driven over unprotected cables or installations.

15. Excavator and loader operators shall not remove the window on the boom side of the operator cab and shall not extend any part of their body outside through this side. If the relevant window is broken, the machine shall not be operated until the window has been replaced.

**MATERIAL STACKING**

1. Loads on transport vehicles shall be securely fastened and shall not be stacked excessively high in order to prevent shifting and overturning.

2. Materials shall not be stacked higher than 3 meters within the construction site. The load-bearing capacity of the floor, ground slope, proximity to excavation edges, type of material, and protection against fire shall be taken into consideration.

[bookmark: _GoBack]3. Materials shall not be stacked in front of passages, roads, fire-fighting equipment, or electrical installations.
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