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1. Before using the lawn mower, read the operating and maintenance manual and follow the instructions.
2. Check the location of the emergency stop buttons and make sure they are functioning properly.
3. Use the provided Personal Protective Equipment (PPE).
4. Check that the machine guards preventing chips or parts from being ejected are complete and properly installed.
5. Before using the machine, be sure to read the operating and maintenance manual and keep it readily available at all times.
6. Do not hesitate to consult your supervisor about anything you do not understand.
7. Do not wear loose or dangling work clothing.
8. Transport and store fuel only in approved and properly marked containers.
9. Do not work alone; keep another employee within calling distance in case of an emergency.
10. Never use the equipment without its protective cover.
11. Before starting the machine, make sure that the cutting tool does not come into contact with hard objects such as branches, stones, etc.
12. Use the machine only with the carrying harness and adjust the harness properly before starting work. The carrying harness must be adjusted to fit the body properly to work without excessive fatigue. Never operate the brush cutter with one hand.
13. Use the brush cutter only under suitable lighting and visibility conditions.
14. During the winter season, be careful of slippery and wet surfaces, ice, and snow. Maintain a safe stance.
15. Do not perform cutting operations above shoulder height. Never use the machine while standing on a ladder.
16. Never climb onto trees to operate the brush cutter.
17. Never work on unstable surfaces.
18. Remove foreign objects, such as stones, from the cutting area.
19. Before storing the brush cutter for an extended period, always empty the fuel and oil tanks.
20. Do not keep fuel-filled brush cutters near fuel filling areas or similar locations.
21. After stopping the machine, begin maintenance, repair, or cleaning operations.
22. Do not leave the machine unattended while it is running.
23. Do not work in a disorderly manner. Do not leave materials on the ground that could cause you to trip and fall.
24. Always hold the brush cutter with both hands during operation. Always maintain a firm and stable stance.
25. Stop the engine during transportation or when moving the machine.
26. The lawn mower shall be operated by only one person and only outdoors.
27. Do not wear accessories or clothing that may become caught in bushes or shrubs.
28. Wear a face shield to protect against sawdust and flying objects generated during cutting.
29. Smoking and the use of open flames are prohibited.
30. Do not refuel while the engine is running.
31. Do not spill fuel or oil on the ground.
32. If fuel spills onto your clothing, change the clothing.
33. Do not refuel indoors.
34. Tighten the fuel tank cap securely and regularly check it for leaks.
35. Begin work at least 3 meters away from the area where the fuel was filled.
36. Fuel cannot be stored indefinitely. Purchase only the amount of fuel that will be consumed in the near future.
37. Make sure that guards for moving parts (belts, pulleys, gearbox, etc.) are properly installed.
38. Wear hearing protection to protect against noise.
39. Wear gloves and steel-toe safety footwear.
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