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1. Cranes shall only be operated by licensed and authorized crane operators specifically assigned to operate the respective crane.

2. No person other than the operator shall be allowed in the operator’s cab.

3. The aerial work platform (basket crane) shall be maintained regularly and without interruption.

4. Personnel working inside the basket shall be provided with all necessary personal protective equipment, including a safety helmet, protective goggles appropriate to the task, a safety harness, and a lanyard for securing themselves to the basket.

5. A barrier shall be installed around the work area, covering the full operating radius of the crane.

6. The crane outriggers shall be properly positioned and adjusted, and it shall be ensured that they are placed on a firm and stable surface.

7. Personnel working in the aerial work platform shall be securely attached to the basket.

8. Personnel inside the basket and the crane operator shall maintain continuous communication, either visually or by radio.

9. Unauthorized personnel shall be prevented from entering the work area, and the necessary precautions shall be taken.

10. The operator shall comply with every stop signal.

11. Work with the aerial work platform shall not be carried out during stormy, overcast or rainy weather conditions.

12. The crane shall never be positioned near high-voltage power lines.
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