

	[image: ]
	YOZGAT BOZOK UNIVERSITY
CIRCULAR SAW OPERATING INSTRUCTION
	
Documan Number: KYT-TLM-014
Publication Date: 20.08.2024
Revision Date:: 
Page No: Page 1 / 1




1. Do not touch the rotating saw while the machine is running.
2. Always use a push stick when cutting short and narrow workpieces.
3. Persons operating the circular saw must be experienced in its use.
[bookmark: _GoBack]4. Do not feed curved, knotty, or nailed pieces into the machine.
5. Do not allow waste pieces to accumulate on the table during operation. Remove accumulated pieces by pushing them away with a wooden stick, not by hand.
6. Always use a feather board when processing thin workpieces.
7. Never pull back the workpiece being cut; if necessary, stop the machine first.
8. Do not operate the machine with the protective guard removed.
9. Do not perform cutting without properly positioning the workpiece against the fence.
10. Do not take measurements while the saw is running.
11. Do not adjust or tamper with the saw settings while the saw is running.
12. After switching the saw to the stop position, do not use any object to rub against the saw in an attempt to stop it immediately.
13. Do not attempt to cut material with a stationary saw.
14. Take care to ensure that the cut piece does not strike the rotating saw after being cut.
15. During cutting, hold the workpiece with your left hand and do not leave the piece unsupported.
16. Take the necessary precautions to prevent sparks generated during cutting from causing damage to the surrounding area.
17. Before starting the cutting operation, make sure that there are no combustible or flammable materials in the vicinity.
18. The saw must rotate in the forward direction. Do not cut with a saw rotating backward; switch it off immediately.
19. Safety goggles and a face shield must be worn when working with a circular saw.
20. Gloves must be worn when working with a circular saw.
21. Position the workpiece to be cut securely and stably.
22. If there is a guard between the workpiece and the operator, it must be positioned so that it does not obstruct visibility.
23. When manually moving the material to be cut, ensure that your hands are sufficiently far away from the circular saw.
24. Do not leave the cut piece unsupported, as it may be thrown or ejected during the final stage of cutting.
25. Install suitable shielding to prevent chips generated during cutting from scattering around.
26. A circular saw with broken teeth must be replaced immediately.
27. If the circular saw teeth have become dull, the saw must be replaced.
28. Do not leave the machine until the saw has completely stopped moving.
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