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1. The Personal Protective Equipment (PPE) to be used shall be determined by the OHS Department based on the risk assessment and the conditions existing on site, and submitted to the Site Manager for approval.
2. Equipment issued for use shall be recorded in the Personal Protective Equipment List.
3. If PPE not included in the list is required, the Site OHS Officer shall be informed. The equipment shall be purchased after it has been added to the list.
4. The selected PPE shall be tried on by the person or team who will use it, and their opinions shall be obtained. The decision to purchase the PPE shall be made based on the feedback received.
5. Practical training on the use of PPE shall be provided by the Site OHS Officers to the personnel who will use the equipment. Equipment-use training shall be repeated whenever the equipment, raw material, or user changes.
6. All PPE shall be suitable for preventing the relevant risk without itself creating an additional risk.
7. Where multiple risks exist and more than one item of PPE must be used simultaneously, the PPE shall be compatible for use together.
8. The duration of PPE use shall be determined by the Site OHS Officer based on the degree of risk, frequency of exposure, nature of the work, and type of PPE.
9. Ergonomics: All PPE shall be provided in accordance with the existing workplace risk conditions and the health status and ergonomic requirements of the worker.

B) TRAINING AND INFORMATION

1. Each employer and subcontractor shall inform their workers about the risks against which the PPE is to be used.
2. The instructions describing the work for which PPE is required shall specify the PPE that must be used.

C) HYGIENE

1. Where PPE intended for use by a single person must, in exceptional circumstances, be used by several people, all necessary measures shall be taken to prevent any health or hygiene problems arising from such use.
2. Once PPE has been issued to an employee for use, that employee shall be responsible for its hygiene.
3. PPE shall be kept in a specially designated area within the site warehouse. When required, the warehouse supervisor shall be contacted. The warehouse supervisor shall be responsible for the cleaning and maintenance of PPE stored in the site warehouse.
   D) SITE PPE USE INSTRUCTIONS, CE MARKING AND CERTIFICATION
4. PPE shall have CE certification, and the CE marking shall also be visibly displayed on the product.
5. Equipment that does not meet the required technical specifications shall under no circumstances be used.

E. PROVISION AND DISTRIBUTION OF PERSONAL PROTECTIVE EQUIPMENT

1. For equipment required for the first time, the Site OHS Officer shall contact the Site Manager and submit a material request. The Site Manager shall implement the Purchasing Procedure in accordance with the request received.
2. PPE shall be provided to employees free of charge by the employer. After maintenance and repair and replacement of any required parts, PPE shall be stored under hygienic conditions in the warehouse and kept ready for use.
3. The Site OHS Officer shall check whether PPE has been delivered to the areas where it is required under site conditions.
4. The Personal Protective Equipment Assignment and Undertaking Form prepared by the OHS Officer at the construction site shall be delivered to the relevant employee receiving the PPE against signature. At the time of delivery, the employee shall be provided with the necessary information regarding the proper use of the PPE and applicable rules.

F) MANDATORY PERSONAL PROTECTIVE EQUIPMENT TO BE USED AT CONSTRUCTION SITES

1. Safety helmets shall be provided to personnel working in areas where objects such as tools, parts, or materials may fall, and the use of safety helmets shall be continuously monitored.
2. Safety harnesses shall be provided to personnel working at heights exceeding 3 meters above the floor where there is a risk of falling or slipping, as well as to roof tile installers, personnel performing gutter and all types of exterior painting work, and operators of winches.
3. Where work requires working in water or concrete, workers shall be provided with suitable rubber boots.
4. Gloves used to protect the hands and arms shall be selected according to the worker's hands and the work to be performed.
5. All personnel working at the construction site, including engineers, architects, technicians, foremen, workers, etc., shall wear steel-toe safety footwear, high-visibility vests, and safety helmets while working on site.
6. PPE provided to electrical workers shall have insulation suitable for the work being performed and the voltage levels to which they may be exposed.
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