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1. The control levers shall only be operated while seated correctly in the operator's cab.
2. Before starting work with the backhoe loader, the controls, brakes, and levers shall be checked.
3. The cab door shall not be left open while the backhoe loader is in motion.
4. Excessively fast or sudden maneuvers shall not be performed.
5. The rear-view mirrors shall be used when maneuvering.
6. The backhoe loader shall never be left unattended while the bucket is raised. The bucket shall be lowered to the ground, the engine shall be switched off, the machine shall be placed in the parking position, and only then shall it be left. The ignition key shall not be left in the machine.
7. Maintenance shall not be carried out underneath the machine by raising and supporting it with the hydraulic lifting cylinders and bucket. For maintenance, the machine shall be taken to a maintenance pit and serviced while in the parked position.
8. Before starting excavation and loading operations, the rear stabilizer legs shall be positioned securely on firm ground, and only then shall work commence.
9. The backhoe loader operator shall continue working only when it is confirmed that the operation is safe. Unsafe or hazardous work shall not be carried out. If the operator detects a hazard during operations, the supervisor shall be informed and work shall be stopped.
10. Long materials shall not be transported in the backhoe loader bucket.
11. The transportation of materials not intended for use in the backhoe loader bucket, such as infrastructure manhole rings, pipes, reinforcing bars, jumpers, etc., is prohibited.
12. Materials in the backhoe loader bucket shall not obstruct the operator's field of vision.
13. Under no circumstances shall people be transported in the backhoe loader bucket.
14. Only the operator is permitted to ride on the backhoe loader. Unauthorized persons shall not be allowed to ride on the machine.
15. The backhoe loader shall not be operated by unauthorized persons.
[bookmark: _GoBack]16. It shall be remembered that compliance with Occupational Health and Safety rules is mandatory during all operations.
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